Neonode zForce(TM) SDK

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
TouchActiveArea Struct Reference

This structure represents the Touch Active Area of a sensor. More...

`#include <zForceTypes.h>`

## Public Attributes
uint32_t | LowerBoundaryX
| Start of the Touch Active Area X axis.
uint32_t | UpperBoundaryX
| End of the Touch Active Area X axis.
bool | HasX
| True if the coordinate system has a X axis.
uint32_t | LowerBoundaryY
| Start of the Touch Active Area Y axis.
uint32_t | UpperBoundaryY
| End of the Touch Active Area Y axis.
bool | HasY
| True if the coordinate system has a Y axis.

## Detailed Description

This structure represents the Touch Active Area of a sensor.

This structure represents the Touch Active Area of a sensor. The Touch Active Area is the area which a sensor will report touches from.

The documentation for this struct was generated from the following file:

- zForceTypes.h